#Create a simulator object

set ns [new Simulator]

#Define different colors for data flows (for NAM)

$ns color 1 Blue

$ns color 2 Red

#Open the NAM trace file

set nf [open out.nam w]

$ns namtrace-all $nf

#Define a 'finish' procedure

proc finish {} {

global ns nf

$ns flush-trace

#Close the NAM trace file

close $nf

#Execute NAM on the trace file

exec nam out.nam &

exit 0

}

#Create four nodes

set n0 [$ns node]

set n1 [$ns node]

set n2 [$ns node]

set n3 [$ns node]

set n4 [$ns node]

#Create links between the nodes

$ns duplex-link $n0 $n2 2Mb 10ms DropTail

$ns duplex-link $n1 $n2 2Mb 10ms DropTail

$ns duplex-link $n2 $n4 1.7Mb 20ms DropTail

$ns duplex-link $n4 $n3 1.7Mb 30ms DropTail

#Set Queue Size of link (n2-n3) to 10

$ns queue-limit $n2 $n4 20

#Give node position (for NAM)

$ns duplex-link-op $n0 $n2 orient right-down

$ns duplex-link-op $n1 $n2 orient right-up

$ns duplex-link-op $n2 $n4 orient right

$ns duplex-link-op $n4 $n3 orient right

#Monitor the queue for link (n2-n3). (for NAM)

$ns duplex-link-op $n2 $n4 queuePos 0.5

#Setup a TCP connection

set tcp [new Agent/TCP]

$tcp set class\_ 2

$ns attach-agent $n0 $tcp

set sink [new Agent/TCPSink]

$ns attach-agent $n3 $sink

$ns connect $tcp $sink

$tcp set fid\_ 1

#Setup a FTP over TCP connection

set ftp [new Application/FTP]

$ftp attach-agent $tcp

$ftp set type\_ FTP

#Setup a UDP connection

set udp [new Agent/UDP]

$ns attach-agent $n1 $udp

set null [new Agent/Null]

$ns attach-agent $n3 $null

$ns connect $udp $null

$udp set fid\_ 2

#Setup a CBR over UDP connection

set cbr [new Application/Traffic/CBR]

$cbr attach-agent $udp

$cbr set type\_ CBR

$cbr set packet\_size\_ 1000

$cbr set rate\_ 1mb

$cbr set random\_ false

#Schedule events for the CBR and FTP agents

$ns at 0.1 "$cbr start"

$ns at 1.0 "$ftp start"

$ns at 4.0 "$ftp stop"

$ns at 4.5 "$cbr stop"

#Detach tcp and sink agents (not really necessary)

$ns at 4.5 "$ns detach-agent $n0 $tcp ; $ns detach-agent $n3 $sink"

#Call the finish procedure after 5 seconds of simulation time

$ns at 5.0 "finish"

#Print CBR packet size and interval

puts "CBR packet size = [$cbr set packet\_size\_]"

puts "CBR interval = [$cbr set interval\_]"

#Run the simulation

$ns run



