.8086

.model small

.data

STR1 db 01h,02h,03h,04h,05h,06h,07h,08h,09h,10h

STR2 db ?

.code

start:

MOV AX, @data

MOV DS, AX

MOV ES, AX

LEA SI, STR1

LEA DI, STR2

MOV CX,0Ah

CLD

REP MOVSB

INT 21h

end start

